Remember to add the following switches to your command
line to load Renegade properly.



RENEGADE -T  - enables Telnet connections with Net2BBS

RENEGADE -TC - enables Telnet connections when used
               with NetSerial or COM/IP.


These switches also set the users baud rate in the
last callers to "TELNET".

Any questions?  Visit the FidoNet Renegade BBS Echo.

            RENEGADE_BBS - FidoNet Tag
