--[ Renegade 05-19.4 released ]------------------------------------------------


 1.  CHANGE -   Updated Copyright notice to reflect the new year.

 2.  FIXED  -   Slight Memory leak in v01-10.4/DOS.  This in turn would
                cause Renegade to eventuatly eat up all availble memory
                in a few years of use if the computer was never rebooted.

 3.  ADDED  -   /F MENUCMD to disable MCI Codes from displaying inside
                of a text file.  This MENUCMD compliments the -F CMD Key.

 4.  ADDED  -   Option /M when entering a message to turn on or off
                using MCI Codes per message.

 5.  ADDED  -   Added option to allow the SysOp access to the amount
                of time to give each timeslice.  This may help some systems
                in which Renegade hogs a lot of CPU (ie: Windows 2000). If
                you do not have much of a problem with sluggish performance
                it is suggested that you leave this option at the default
                setting. (10-40 optimal setting)

                [System Config -> D. System Variables -> V. Time Slices]

 6.  FIXED  -   Slight problem when displaying "NEW" bulletins to users
                when they first logon.  Renegade would display 22 of them
                across, then start putting each new one on a new line.

 7.  REMOVE -   Removed "Digiboard" support in the codebase.  Really,
                who would use one of those now-a-days anyways with a DOS
                based BBS?  If this is an issue for anyone, please e-mail
                us and we'll take care of it for you.

 8.  ADDED  -   Added option to System Config to post the BBS's telnet
                URL.  This is under System Conifg, Option A Main BBS Config.
                Just a cosmetic add, as before you could only type in a
                telephone number for the BBS.  Now you have a choice. ;)

 9.  ADDED  -   Added ~TN MCI Code to BBSME.ASC/ANS and BBSMN.ASC/ANS
                to reflect the new Telnet address line to the BBS list.

10.  CHANGE -   Changed the follow command keys to reflect new BBS
                list format change.

                       {  See Below for list of CMD Keys  }

                OB : Changed to CMD Key   TV   {short view of bbslist}
                OA : Changed to CMD Key   TA   {Add to bbslist}

                Added the following CMD Keys to be able to have more
                control over the BBS List.

                TA  : BBSList Add           {formally CMD Key OB}
                TE  : BBSList Edit 
                TV  : BBSList Short View    {formally CMD Key OV}
                TX  : BBSList Extended View {formally CMD Key OV}

                { Updated MENUCMD.ASC file to reflect these changes }

11.  CHANGE -   BBS Listing is now scriptable.  This means that you
                now can add just about any question for the BBS you wish.
                MCI Codes reflect the different questions (1-8) to display
                when a user views the BBS List.

                { Added BBSLIST.SCR file to reflect this update }

                *** BBSLIST.SCR MUST BE IN THE \BBS\MISC DIRECTORY ***

12.  ADDED  -   %xA / %xB / %xC / %xD / %xE / %xF for extra definable
                sysop strings in the BBSLIST.SCR file.

                                x:= to the following values.
                a = 8 chars / b = 30 / c = 30 / d = 40 / e = 60 / f = 60

                Also added %S2 for and extra line of descrition of the
                BBS.  Changed the way it stores the SOFTWARE. It's all
                in capital letters now.  Also, added that if can't find
                BBSMN.ASC it will echo back that in the sysop log and
                just print out the bbslist.sysopname, etc and proceed.

13.  ADDED  -   BBS*.ASC New MCI - ~WS (website) ~RN (Record Number)

14.  CHANGE -   -TG and -TS command line loaders for Renegade are
                now simply just -T for all telnet connections.  Unless
                you are using COM/IP as your emulator which the command
                line changed to -TC (ie: renegade.exe -n4 -tc).

16.  UPDATE -   The Official Renegade Home page is now located at URL:
                              http://www.renegadebbs.net

17.  REMOVE -   Removed the "Moving xx to xx" from writing to the
                SYSOPx.LOG file.  Saved some clutter there. ;)

18.  FIXED  -   The Telnet URL will now save correctly in the
                system config and not constantly erase itself.
                Will have to set for each node.

19.  CHANGE -   Bulletins now compare Time and Date of Files vs Time
                and Date of last logon to display as NEW.

20.  CHANGE -   NODE*.ASC instead of showning a '-' when a user isn't
                on a node it will echo back the node number for ~NN, then
                for ~AV it will display 'Y'. MCI Code ~AC is a 20 Chars
                String and ~UN is a 36 character string.

21.  CHANGE -   The Caller ID switch is now -ID instead of just -I
                Also -IP puts the IP (if present) into the Caller ID field
                in the User Editor and anything to do with Caller ID.

22.  ADDED  -   The String Editor is now removed from Renegade.  All
                strings within the editor are now EXTERNAL.  We will
                slowly be removing all strings from within Renegade's
                code and making them external for easy editing!  Also
                created DUMP to "dump" the STRING.DAT file to the
                editable language file. (data\renegade.lng)


--[ Renegade 01-10.4 released ]------------------------------------------------

  1.  FIXED  - Bulletins - Now will correctly display if a bulletin
               is new or not to the user per call and are sorted
               in numerical order.  ie: (2, 7, 19, 22) instead of
               (22, 2, 19, 7).

  2.  ADDED  - (-T, /T) Toggle.  This will inturn toggle all baud
               rate speeds to show as "TELNET".  This also disables
               most comm routines relating to logoffs.  With -T
               added to loading Renegade, it will no longer pause
               for a set number of seconds before the BBS will
               hang the user up.  DO NOT use this command on
               dialup nodes!  Use this on TELNET ONLY NODES!!!!

   3. REVISED  (-T, /T) (-TG, /TG) (-TS, /TS) Load Toggle.
               This will inturn toggle the MCI Code ~SP in
               the last caller ANSI/ASCII to show 'BAUD'.
               (-T, /T) will do the hang-up procedure on a
               regular log-off for COM/IP.  (-TG, /TG) & (-TS, /TS)
               will bypass the passing of the ATH0 hangup string
               to the fossil/com port and will work with GameSrv
               or Synchronet respectivly.  This fix's issues of
               slow hangups while doing a telnet session.
               DO NOT use this command with dialup nodes!

   3. FIXED  - Fixed Toggles Menu and added warning screen about
               the use of certain toggles and what else should be
               changed or certain users may not be able to log
               back on to the BBS.  (ie:  If you have the BBS
               check for birthday's and have the toggle to ask
               for the birthday at new logon set to NO, the user
               will not be able to logon the BBS since he will not
               have a birthday set in the user record.)

   4. FIXED  - Added Time Slice Routines to certain functions in
               Renegade where it awaits for a user input.  This
               SHOULD fix some slow downs while running under
               some version of Windows.

   5. FIXED  - Fixed Memory problems with downloads and swapping
               Renegade out of memory which in turn caused some
               doors not to function.

   6. CHANGE - Changed all file sizes in Renegade to now show as
               Kilobyte (KB), and Megabytes (MB) instead of just
               bytes. (ie: 64,564 bytes NOW DISPLAYS AS 64.5 KB)
               Also changes to the WFC Screen to reflect this.

   7. FIXED  - Fixed upload Limit of 8.1 MB.  Now, will show
               files with sizes up to 1.9 GB.

   8. FIXED  - Fixed the AR, AC Flags [- OF -] toggle command to
               NOT be case sensitive.

   9. ADDED  - MCI Code telnet - This MCI Code shows the users speed,
               ie: Telnet, Local, or Actual Baud Rate.



